Looking at the PRR#1169, it appears that participating load that is use limited providing RA by non-spin per tariff section 40.6.4.3 is not anymore in the BPM for reliability requirement. Is this being eliminated or just an error?

A participating load meets RA by offering non-spin in the IFM and energy bid to drop load in RTM for IFM non-spin award as stated in the tariff section 40.6.4.3 specifying how a participating load can meet RA and has different DAM and RTM must offer obligation in terms of what needs to be offered compared to other generating units. It would make this tariff requirement clearly stated in the BPM by setting specific requirement for a participating load (non-spin in DAM and energy drop in RTM for DAM A/S award) compared to a generator (requirement energy, A/S, RUC etc.). Otherwise, the general requirement for use limited resources would mask the specific requirements from a participating load (PL) even though the tariff allows RA from a PL by offering non-spin. This would certainly add clarity in the BPM.